|  |
| --- |
| NETWORK COMMUNICATOR  (CONTROL FLOW) |
| Client server relation is established through a network. |
| Each host (server/client) is assigned a unique local IP address. |
| The host sends a data packet to another host by addressing its IP address. This is the case when Client requests a specified data/processes. |
| The recipient host identifies the sender by its IP address. |
| Hence the Server relays the process output to the Client. |